**PlexPi** is a ready-to-deploy, optimized and current Plex Media Server for Raspberry Pi 3 Microcomputers.

The name “PlexPi” is not necessarily the final name of the project since I feel there would be benefit to making this compatible with other boards such as the ODROID XU4. But that said, DietPi gets away with it, so maybe PlexPi is a good name.

**System Requirements (1.3+):**

* Raspberry Pi 3 Model B or B+ (PlexPi 1.3+ is required for B+)
* 16 GB+ MicroSD Card (8 GB+ for PlexPi 1.0-1.2)

**Access PlexPi from any computer on LAN:**

<http://plexpi.local:32400/web>

**SSH Access:**

plexpi.local

Username: pi

Password: plexpi1

**Access Desktop:**

To close the kiosk screen after booting (and thereby access the desktop) simply press ALT-F4 on a keyboard attached to the Pi.

**Please report any issues** [**in the community forum**](http://forum.category5.tv/forum-46.html)**.**